SDS Section 2 Workplace Review

Using hazard classifications to review workplace tasks
Use the checklist for the exact product and proposed U.S. workplace operation. It is a recommended review aid, not an OSHA-prescribed approval certificate. Record evidence and unresolved questions; a checked box does not replace the applicable assessment.
Workplace review checklist
Product and SDS revision: [Identify]. Task/location: [Identify]. Reviewer/date: [Identify].
	Verification point
	Yes, No, or N/A with evidence

	Container identifier, supplier, grade, and component match the reviewed SDS
	[Result and evidence]

	Every applicable health and physical hazard is read, including class/category and hazard statements
	[Result and evidence]

	Signal-word or pictogram precedence is not treated as removal of other listed hazards
	[Result and evidence]

	HNOCs, reaction-product hazards, and any required unknown-acute-toxicity information are reviewed
	[Result and evidence]

	Intended use, transfer, application, cleanup, and maintenance are defined
	[Result and evidence]

	Exposure routes and affected workers are identified
	[Result and evidence]

	Sections 3, 7, 8, 9, 10, and 11 support the task review; important inconsistencies are resolved
	[Result and evidence]

	Actual storage, incompatibilities, and ignition conditions are evaluated
	[Result and evidence]

	Selected controls and PPE have a task-specific basis; required respiratory arrangements are complete
	[Result and evidence]

	Applicable emergency washing, release response, and communication arrangements are established
	[Result and evidence]

	Required information, training, and access to SDSs/labels are established
	[Result and evidence]

	Applicable industry, State Plan, HCS transition, and substance-specific requirements are considered
	[Result and evidence]



Essential missing information or control: [Describe]. Owner and work restriction: [Identify].
Disposition: [ ] Hold. [ ] Separate controlled trial review. [ ] Accept defined conditions. [ ] Reject proposed use.
Decision authority/date and limits: [Identify].
Classification to task decision record
Duplicate this record for each materially different hazard or operation. Keep product classification separate from employee exposure estimates.
	Decision field
	Entry

	Product, revision, hazard class/category, and relevant statement
	[Identify source information]

	Actual task and hazardous condition
	[Describe]

	Exposure routes and affected people
	[Identify]

	Assessment question
	[What must be established?]

	Related SDS information and technical evidence
	[Sections and record references]

	Governing requirement versus recommended company practice
	[Identify each accurately]

	Selected control and its verification
	[Describe evidence, not just installation status]

	Information still needed
	[Supplier question or technical review]

	Decision and operating limits
	[Hold/accept/reject and actual scope]

	Reviewer, authority, and date
	[Identify]



Example review cues
For a flammable product, assess actual release, ignition, equipment, and storage conditions; a flame pictogram is not a ventilation design. For a corrosive product, assess contact opportunities, protective equipment, handling configuration, and applicable emergency washing. For sensitization or target-organ effects, identify relevant routes and exposure evidence. Do not infer one PPE kit from a signal word.
Reassessment triggers: product or formulation change, changed task/application, new hazard information, exposure findings, inadequate controls, or worker concerns. Record any immediate protective action separately from the administrative review.
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